|  |  |  |  |
| --- | --- | --- | --- |
| **No**  |  **Name of Maintenance Tools & Equipment**  |  **Unit**  | **Total Qty.** |
|  |
|  |
|  |
|  |
|  1.00  |  **Hydraulic Press for Conductor**  |  |  |  |
|   |  120 Ton Hydraulic press for conductor and earth wire with two set of dies (12, 14, 16, 18, 20, 22, 24, 26, 30, 32, 34, 36, 38, 40, 45, 50mm)  |  Set  | **12** |  |
|  2.00  |  **Hydraulic Opraed ACSR and others Conductor Cutter**  |  |  |  |
|   |  Hydraulically operated ACSR and others Conductor cutter suitable for cutting the ACSR conductor up to 45mm diameter along with the required sizes blades hand pump, hose pipe and other accessories . The cutter shall be providede with spares  |  Set  | **12** |  |
|  3.00  |  **Tirfor**  |  |  |  |
|   |  Trifor pulling capacity 5 Ton  |  Each  | **18** |  |
|  Trifor pulling capacity 8 Ton  |  Each  | **18** |  |
|  Trifor pulling capacity 10 Ton  |  Each  | **18** |  |
|  4.00  |  **Self Gripping Clamps**  |  |  |  |
|   |  Self Gripping Clamps for 400 and 500KV Transmission line conductor  |  Each  | **42** |  |
|  5.00  |  **Naylon rope**  |  |  |  |
|   |  Naylon rope Ø 14 mm 300mt  |  each  | **36** |  |
|   |  Naylon rope Ø 16 mm 300mt  |  each  | **36** |  |
|   |  Naylon rope Ø 18 mm 300mt  |  each  | **36** |  |
|  Naylon rope Ø 20 mm 300mt  |  each  | **36** |  |
|  Naylon rope Ø 24 mm 300mt  |  each  | **36** |  |
|  6.00  |  **Polyester Webbing Sling both End eye type**  |  |  |  |
|   |  Polyester Webbing Round Slings 1mt-5ton capacity  |  each  | **36** |  |
|  Polyester Webbing Round Slings 2mt-5ton capacity  |  each  | **36** |  |
|  Polyester Webbing Round Slings 3mt-5ton capacity,  |  each  | **36** |  |
|  Polyester Webbing Round Slings 1mt-8ton capacity  |  each  | **36** |  |
|  Polyester Webbing Round Slings 0.5mt-8ton capacity,  |  each  | **36** |  |
|  Polyester Webbing Round Slings , 2mt-8ton capacity,  |  each  | **36** |  |
|  Polyester Webbing Round Slings 10mt-12ton capacity,  |  each  | **36** |  |
|  Polyester Webbing Round Slings 3mt-20ton capacity,  |  each  | **36** |  |
|  Polyester Webbing Round Slings 6mt-20ton capacity,  |  each  | **36** |  |
|  Polyester Webbing Round Slings 12mt-20ton capacity,  |  each  | **36** |  |
|  7.00  |  **Lever Chain Hoist**  |  |  |  |
|   |  Lever Chain Hoist 5 Ton  |  Each  | **9** |  |
|  Lever Chain Hoist 10 Ton  |  Each  | **18** |  |
|  8.00  |  **Chain Block Hoist**  |  |  |  |
|   |  Chain Block Hoist 5Ton  |  Each  | **18** |  |
|   |  Chain Block Hoist 8Ton  |  Each  | **18** |  |
|  9.00  |  **Steel Wire Rope Slings both end spliced**  |  |  |  |
|  |  |  |  |  |
|   |  10mm2x2 meter  |  Each  | **18** |  |
|   |  12mm2x3 meter  |  Each  | **18** |  |
|  12mm2x1.5 meter  |  Each  | **18** |  |
|  16mm2x3 meter  |  Each  | **18** |  |
|  16mm2x1.0 meter  |  Each  | **18** |  |
|  10.00  |  **Service Pulley**  |   |  |  |
|   |  Service snatch sagging blocks in steel (3 ton) wire diameter 10-14 mm  |  Each  | **36** |  |
|  Service snatch sagging blocks in steel (6 ton) wire diameter 14-20mm  |  Each  | **36** |  |
|   |  Service snatch sagging blocks in steel (6 ton) wire diameter 16-22mm  |  Each  | **36** |  |
|   |  Service snatch sagging blocks in steel (6 ton) wire diameter 20-25mm  |  Each  | **36** |  |
|  11.00  |  **Closed type Single Sheave Pulley**  |  |  |  |
|   |  5ton capacity -12mm steel rope  |  Each  | **36** |  |
|  2.5ton capacity -12mm steel rope,  |  Each  | **36** |  |
|  12.00  |  **Two sheave pulley**  |  Each  |  |  |
|   |  Two sheave pulley wire rope diameter 16-20mm  |  Each  | **36** |  |
|  13.00  |  **Four sheave pulley**  |  Each  |  |  |
|   |  Four sheave pulley 5 ton capacity for wire rope diameter 14-16mm.  |  Each  | **36** |  |
|  Four sheave pulley 10 ton capacity wire rope diameter 16-20mm  |  Each  | **36** |  |
|  14.00  |  **Different types of Wrench 10-50mm2**  |  **Set**  | **18** |  |
|  15.00  |  **Motorized Inspection Trolleys**  |  |  |  |
|   |  Inspectio Trolley for two bundle conductors  |  Each  | **9** |  |
|  16.00  |  **Jin pole**  |  |  |  |
|   |  Jin pole of adjustable height from 4-12 mt. maximum lifting capacity 2 ton (4+4+4)  |  Each  | **9** |  |
|  17.00  |  **Binocular**  |  |  |  |
|   |  Zoom binoculars with magnifying power of 8 - 20 times, out doors type, water resistance, suitable for focussing the objects from a distance of 1000 metres.  |  Each  | **24** |  |
|  18.00  |  Grainder machine  |   |  |  |
|   |  portable Electrical Hand Grinder  |  Set  | **9** |  |
|  19.00  |  **Chain Saw Machine/ Wood Cutting Chain Saw Machine**  |  |  |  |
|   |  Chain Saw Machine/ Wood Cutting Chain Saw Machine  |  Set  | **18** |  |
|  20.00  |  **Aluminum alloy sliding ladders hook ends**  |  |  |  |
|   |  Aluminum alloy ladders of 15mts length  |  Set  | **18** |  |
|  21.00  |  **Voltage detector**  |  |  |  |
|   |  For 132 upto 500 kv  |  Set  | **24** |  |
|  22.00  |  **Grounding device for safety purpose**  |  |  |  |
|   |  Grounding device designed for conductor tobe used during stringing operation on 132, 230 kv, 400kv and 500kv high voltage transmission lines  |  Set  |  |  |
|  For 2300 kv  |  Set  | **12** |  |
|  For 400 kv  |  Set  | **7** |  |
|  For 500 kv  |  Set  | **5** |  |
|  23.00  |  **VHF Portable Radio**  |  |  |  |
|   |  Walki -Talki portabl radios up to 25 km covering & with rechargeable batteries with individual charging unit  |  Set  | **24** |  |
|   |  VHF Base radio  |  Set  | **24** |  |
|  24.00  |  **Welding Machine**  |  |  |  |
|   |  Single phase Portable Welding Machine  |  Set  | **12** |  |
|  Three Phase Diesel Welding Generator • Current Range (Continuous) 20 - 400AWith welding pliers and accessory  |  Set  | **12** |  |
|  Argon arc welder With welding pliers and accessory  |  Set  | **12** |  |
|  25.00  |  **Drill machine**  |  |  |  |
|   |  Heavy duty motor operated drill machine with stand and bits of 6mm,12mm,16mm ,20mm  |  Set  | **12** |  |
|  26.00  |  **Hydraulic Crimping Tools**  |   |  |  |
|   |  Hydraulic Crimping Tools 12Ton  |  Each  | **12** |  |