**TECHNICAL SPECIFICATION FOR HYDRAULIC PALLET TRUCK TROLLEY**

|  |  |  |
| --- | --- | --- |
| **Ser** |  **Nomenclature & Specification** | **Your Requirement** |
| 1. | **Hydraulic Pallet Truck Trolley with all standard and additional accessories as per specification below:** | **Hydraulic Pallet Truck Trolley with all standard and additional accessories as per specification below:** |
| 2. | Model : To be mentioned | Model : HPT03B |
| 3. | Purpose: This trolley is for internal transportation of components and other goods. | Purpose: same as left |
| 4. | **specification :**  | **specification :**  |
| a. Capacity: 3000 kg | a. Capacity: 3t |
| b. Maximum Fork Height: 190 ~ 200 mm | b. Maximum Fork Height: 190mm |
| c. Maximum Fork Height: 75 ~ 85 mm | c. Maximum Fork Height: 82mm |
| d. **Fork Dimension**: | **Fork Dimension**: |
|  (1) Length: 1200 Distance between  Two Forks: 1200 ~ 1300 mm | (1) Length: 1220 mm |
|  (2) Width: 150 ~ 160 mm  | (2) Width: 160 mm  |
|  (3) Distance between Two Forks (Center to Center): 370 ~ 380 mm | (3) Distance between Two Forks (Center to Center): 365 mm |
|  (4) Thickness of Fork Sheet Material: 5 mm  (minimum) | (4) Thickness of Fork Sheet Material: 4 mm |
|  (5) Load Roller Diameter: As Standard  (mention the size) |  (5) Load Roller Diameter: φ80\*68 |
|  (6) Steering Wheel Diameter: As Standard  (mention the size) | (6) Steering Wheel Diameter: φ180\*50  |
|  (7) Wheel: Double Wheel Nylon/Poly Urethane | (7) Wheel: Nylon wheel |
| **Country of Origin: Group B** |
| Conditions: |
| a. all Standard attachment and necessary accessories must be supplied with the Trolley. |
| b. Year of manufacture: Not earlier than year of signing the contract. |
| c. Trial rum should be done by the supplier. |
| d. 1 x Operating Manual/Programming Manual in English must supplied with Trolley. |
| e. 2x Maintenance/Repair Manual in English must supplied with the Trolley. |
| F. Bidders should submit original leaflet/Brochure with the offer. |
| g. 02 set spare wheel must supply with each trolley. |
| h. Warranty: 01 year after acceptance. |
| j. Standard lubricating system should be |