|  |  |  |  |
| --- | --- | --- | --- |
| **No.** | **Item** | **Manufacturer** | **Place of Manufacture/Inspection** |
| 01 | 3T Chain Hoist | **RAMHOIST** | **CHINA** |
| 02 | 6T Chain Hoist | **RAMHOIST** | **CHINA** |
| 03 | 9T Chain Hoist | **RAMHOIST** | **CHINA** |

|  |  |  |
| --- | --- | --- |
| **OPTION** | **CEB REQUIREMENT** | **OFFERED**  |
| Name of manufacturer | Mention Themanufacturer name | Nanjing RAM Machinery co.,ltd |
| Country of origin | Mention The country oforigin | china |
| Address of the manufacturer | Mention The address ofthe manufacturer | Building 2, No.8 Songyuan South Road Gaochun Economic Development Zone, Nanjing |
| Color/ Finish  | Mention the color | ORANGE |
| Make and Model  | Mention Make and Model | VA03, VA06, VA09 |
| **3 Ton Chain Hoist** |  |  |
| Rated load  | 3 Ton | 3 Ton |
| Chain length  | More than 1.5 m | 1.5 M |
| Net weight of hoist  | Maximum 22 kg | **17.5kg** |
| Force on handle at max. load  | Less than 0.33 kN | **320N** |
| Length of the Handle  | Around 410 mm | 410MM |
| **6 Ton Chain Hoist** |  |  |
| Rated load  | 6 Ton | 6 Ton |
| Chain length  | More than 1.5 m | 1.5 M |
| Net weight of hoist  | Maximum 32 kg | 28.5KG |
| Force on handle at max. load  | Less than 0.35 kN | **340N** |
| Length of the Handle  | Around 410 mm | 410MM |
| **9 Ton Chain Hoist** |  |  |
| Rated load  | 9 Ton | 9 Ton |
| Chain length  | More than 1.5 m | 1.5 m |
| Net weight of hoist  | Maximum 50 kg | 45kg |
| Force on handle at max. load  | Less than 0.37 kN | **360N** |
| Length of the Handle  | Around 410 mm | 410MM |
| Snatch hooks | Snatch hooks are required for all loading and connecting hooks | Snatch hooks |
| Hoist made of  | All steel construction | All steel construction |
| Chain made of | Electro zinc plated load chain | Electro zinc plated load chain |
| Hooks made of | Forged alloy steel hooks with cast steel safety latches | Forged alloy steel hooks with cast steel safety latches |
| Overload protection | Overload protectionmechanism is required | **With** Overload protection |
| Service level | Heavy service level asmentioned in the tenderdocument | yes |
| Rotation provision of loading and connecting hooks | 360 degree required | yes |
| ISO 9001 for manufacturer | Yes/No | yes |
| Manufactures technical literature | Provided/Not Provided | Provided |
| Warranty period | 12 months after deliveringto CEB | Warranty period 12 months |
| Delivery period | Within 12 weeks afteraward date |  45 days after received deposit |
| Documents | All the operational andmaintenance manuals arerequired | operational andmaintenance manuals can offer |